­­­*End Cap Installation Instructions*

*Gutter Topper® end caps are designed to fit and work with Gutter Topper®. To install the end cap, first make sure the piece will fit into the gutter. If the end cap is too large to fit securely in the gutter, you will have to trim off some excess from the BACK of the piece. Use caution that you do not trim off too much as that will result in the end cap not covering the open area.*

*Position the end cap between the end of the gutter and the gutter protection with the colored side toward the end of the gutter. The top piece, which is perpendicular to the gutter, should be positioned UNDER the gutter protection. The front nose of the product and the front of the end cap should be in alignment. Insert two 1/4/ inch zip screws into the top of the gutter protection, effectively tying the gutter protection to the end cap.*

*(See illustration D)*

 ↓ ↓

Zip Screws on top

Front Nose of product

Front nose of end cap

A picture containing roof

Description automatically generated